(kicad_pcb (version 20221018) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")
  (net 1 "unconnected-(PS1-AC{slash}L-Pad1)")
  (net 2 "unconnected-(PS1-AC{slash}N-Pad3)")
  (net 3 "unconnected-(PS1-NC-Pad5)")
  (net 4 "unconnected-(PS1--Vo-Pad14)")
  (net 5 "unconnected-(PS1-+Vo-Pad16)")

  (footprint "Converter_ACDC:Converter_ACDC_MeanWell_IRM-03-xx_THT" (layer "F.Cu")
    (tstamp 7e0f7215-bd6f-4b1d-98e0-460c58ebcb10)
    (at 92.71 86.995)
    (descr "ACDC-Converter, 3W, Meanwell, IRM-03, THT, https://www.meanwell.com/Upload/PDF/IRM-03/IRM-03-SPEC.PDF")
    (tags "ACDC-Converter 3W THT")
    (property "Sheetfile" "pso.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "12V, 250mA, 3W, Isolated, AC-DC, IRM03")
    (property "ki_keywords" "Miniature Module-type Power Supply MeanWell")
    (path "/3645a35f-038d-4e94-a5da-8babbe5ed916")
    (attr through_hole)
    (fp_text reference "PS1" (at 8.89 -4.5) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 521469e0-86a8-4ee1-97e9-fb26fe54237f)
    )
    (fp_text value "IRM-03-12" (at 8.89 16.24) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 721f6a06-f706-4bf2-bc86-3ee4854d7a1c)
    )
    (fp_text user "${REFERENCE}" (at 8.89 14.24) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2383721a-515f-4f33-ba4b-447cb12821f1)
    )
    (fp_line (start -3.61 -2) (end -3.61 4)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fc3c5bbb-d173-4697-b33a-225cd9eab970))
    (fp_line (start -3.23 -3.38) (end -3.23 33.86)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 37528b16-199a-4758-bd6d-6aa80153e387))
    (fp_line (start -3.23 33.86) (end 21.01 33.86)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1b411b91-0d18-4232-994b-4b3d4aa913ed))
    (fp_line (start 21.01 -3.38) (end -3.23 -3.38)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp eb59a896-fef5-4486-b3da-eed101db4474))
    (fp_line (start 21.01 -3.38) (end 21.01 33.86)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c3ee9901-5fc8-4ad9-93b2-686a55c5c75a))
    (fp_line (start -3.36 -3.51) (end -3.36 33.99)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1b8578e7-c1c2-42d0-83b5-1589d9374b36))
    (fp_line (start 21.14 -3.51) (end -3.36 -3.51)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 28618584-d45f-4a44-b883-54d0abe98dc5))
    (fp_line (start 21.14 -3.51) (end 21.14 33.99)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c88c56ba-5a60-49c9-81e1-fe041c7ab68d))
    (fp_line (start 21.14 33.99) (end -3.36 33.99)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d5df98db-47bd-4dd5-b63f-bb9cdb636840))
    (fp_line (start -3.11 -1) (end -3.11 -3.26)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bcd851ab-1523-4ee9-a26a-f71c0b250821))
    (fp_line (start -3.11 1) (end -3.11 33.74)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e4faeaa1-5a01-4503-893e-24b1930ae695))
    (fp_line (start -3.11 1) (end -2.11 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0cd6a31a-801d-46f7-ac99-a076688ba6a1))
    (fp_line (start -2.11 0) (end -3.11 -1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e286cced-ad79-40ca-9ed3-c5623d593fa3))
    (fp_line (start 20.89 -3.26) (end -3.11 -3.26)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7726ed5e-d8e1-47d1-bb6b-d418527412e2))
    (fp_line (start 20.89 -3.26) (end 20.89 33.74)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d1506a8f-0fee-4991-8ebe-906b186dd7aa))
    (fp_line (start 20.89 33.74) (end -3.11 33.74)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6ecceae6-309e-4ef9-b091-0f849a47892b))
    (pad "1" thru_hole rect (at 0 0) (size 2.3 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "unconnected-(PS1-AC{slash}L-Pad1)") (pinfunction "AC/L") (pintype "power_in") (tstamp b29a8144-e8a6-408e-b584-61012a22c083))
    (pad "3" thru_hole circle (at 0 5.08) (size 2.3 2.3) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "unconnected-(PS1-AC{slash}N-Pad3)") (pinfunction "AC/N") (pintype "power_in") (tstamp 7d54d9c2-d135-4a90-abe9-d89f97cea1e2))
    (pad "5" thru_hole circle (at 0 30.48) (size 2.3 2.3) (drill 0.76) (layers "*.Cu" "*.Mask")
      (net 3 "unconnected-(PS1-NC-Pad5)") (pinfunction "NC") (pintype "no_connect") (tstamp b74036ca-60c5-4937-a684-fcbadfb14462))
    (pad "14" thru_hole circle (at 17.78 30.48) (size 2.3 2.3) (drill 0.76) (layers "*.Cu" "*.Mask")
      (net 4 "unconnected-(PS1--Vo-Pad14)") (pinfunction "-Vo") (pintype "power_out") (tstamp 1cacf5a2-ded1-412b-8ba2-ee7a082b9a4c))
    (pad "16" thru_hole circle (at 17.78 25.4) (size 2.3 2.3) (drill 0.76) (layers "*.Cu" "*.Mask")
      (net 5 "unconnected-(PS1-+Vo-Pad16)") (pinfunction "+Vo") (pintype "power_out") (tstamp 4460e1be-2f91-4574-8134-5f1ea7759afd))
    (model "${KICAD6_3DMODEL_DIR}/Converter_ACDC.3dshapes/Converter_ACDC_MeanWell_IRM-03-xx_THT.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

)
