(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(J1-Pin_2)")
	(net 2 "GND")
	(net 3 "Net-(J1-Pin_3)")
	(net 4 "Net-(Q3-G)")
	(net 5 "Net-(J1-Pin_4)")
	(net 6 "Net-(BT1-+)")
	(net 7 "unconnected-(U2-XTAL1{slash}PB3-Pad2)")
	(net 8 "Net-(J2-Pin_1)")
	(net 9 "Net-(J2-Pin_3)")
	(net 10 "Net-(J2-Pin_4)")
	(net 11 "Net-(J2-Pin_5)")
	(net 12 "Net-(J2-Pin_6)")
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(uuid "22db4a31-6da7-4c0c-8b76-28c75d0c66d6")
		(at 104.95 89.0625 90)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q2"
			(at 0 -2.4 90)
			(layer "F.SilkS")
			(uuid "d4be787c-a42d-454a-b36e-f2bc51daaeb8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "IRLML6244"
			(at 0 2.4 90)
			(layer "F.Fab")
			(uuid "308f1cd5-c681-4be9-9b84-2848eae1e0a8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0fe1a9d3-29d6-446b-9b85-224ae2fb8943")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "80477dc7-0f6d-43d5-961d-0efa6a9d937b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "30A Id, 50V Vds, N-Channel Power MOSFET, TO-220"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3758bf25-b81d-4045-803d-5c7393e80314")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/b5f3fa48-69ca-4b7b-8318-5560f5faba53")
		(sheetfile "led-controller.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -1.56)
			(end 0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "718aaf1b-b0b1-4999-a7e3-5d0d2011cb5a")
		)
		(fp_line
			(start 0 -1.56)
			(end -0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7c385310-2ec0-40b2-93dc-f9bc718b0d48")
		)
		(fp_line
			(start 0 1.56)
			(end 0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "621b0ec0-4d74-4a9f-8b6d-67b6d29e0fbe")
		)
		(fp_line
			(start 0 1.56)
			(end -0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dbdab303-cb52-4520-ace2-4769170173b8")
		)
		(fp_poly
			(pts
				(xy -1.1625 -1.51) (xy -1.4025 -1.84) (xy -0.9225 -1.84) (xy -1.1625 -1.51)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "40be1255-d070-4f0b-8306-00d40d8f33de")
		)
		(fp_line
			(start 1.92 -1.7)
			(end -1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b63826be-769f-4730-a7aa-cb2d0459eb14")
		)
		(fp_line
			(start -1.92 -1.7)
			(end -1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "94b4826b-4e0f-4cb4-93f5-4105117a9e10")
		)
		(fp_line
			(start 1.92 1.7)
			(end 1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3bf57eaf-e923-4366-925d-7752413fbf05")
		)
		(fp_line
			(start -1.92 1.7)
			(end 1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "21ca5232-8f56-42b0-b56a-9b0087440ddf")
		)
		(fp_line
			(start 0.65 -1.45)
			(end 0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4ca5fb78-4024-4dc5-9c5c-c2a39dcc921a")
		)
		(fp_line
			(start -0.325 -1.45)
			(end 0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cd7ff15f-54ef-4d1b-81e1-c803e3630096")
		)
		(fp_line
			(start -0.65 -1.125)
			(end -0.325 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "81cc7f51-c048-4c70-9789-cf2cf118495a")
		)
		(fp_line
			(start 0.65 1.45)
			(end -0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c449d185-f15a-40d6-912d-254c56ef96a5")
		)
		(fp_line
			(start -0.65 1.45)
			(end -0.65 -1.125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b380bad6-1d8c-4b48-923c-8b8d3fe4d7ab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "d339adf3-4d0f-459e-b553-ed7934d22123")
			(effects
				(font
					(size 0.32 0.32)
					(thickness 0.05)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "Net-(J2-Pin_4)")
			(pinfunction "G")
			(pintype "input")
			(uuid "3bce8582-7372-4551-aa88-63dce165f13b")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(J1-Pin_3)")
			(pinfunction "D")
			(pintype "passive")
			(uuid "86ee4059-7a89-4f02-8501-a4ffd3ce23e7")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "S")
			(pintype "passive")
			(uuid "ffbf0462-962b-4c6d-afc2-137f42b0d8d5")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm"
		(layer "F.Cu")
		(uuid "24e5a32f-21e6-4a05-81d7-802e27ca308e")
		(at 111.5 101 180)
		(descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
		(property "Reference" "C1"
			(at 1 -3.75 360)
			(layer "F.SilkS")
			(uuid "b7313153-00ef-49d9-9e94-17ca62e91753")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 1 3.75 360)
			(layer "F.Fab")
			(uuid "f74437b6-a0c7-435f-8fd7-05d0dfe0601a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
			(uuid "22df7154-db91-4b25-b19c-8244a2dc629f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
			(uuid "af6dfc49-8c1d-4dc4-a678-f0b4f4346f55")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
			(uuid "974e5760-6e51-4094-abd9-9e6a597ef6f9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/7d95ce59-bf2f-4a34-b557-2b74dcc46f7f")
		(sheetfile "led-controller.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 3.601 -0.284)
			(end 3.601 0.284)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "eaee9510-7950-4c8b-b52e-1a43d77d49e5")
		)
		(fp_line
			(start 3.561 -0.518)
			(end 3.561 0.518)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e62d514d-5449-4bfa-80a2-77a9bc706016")
		)
		(fp_line
			(start 3.521 -0.677)
			(end 3.521 0.677)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ecc761fa-09c7-4452-9619-36f525247d2d")
		)
		(fp_line
			(start 3.481 -0.805)
			(end 3.481 0.805)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4c42b7ab-98ad-4402-b504-dc7d2d028700")
		)
		(fp_line
			(start 3.441 -0.915)
			(end 3.441 0.915)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "acbedabf-5b23-4cd8-bb8e-c909cf6e64c0")
		)
		(fp_line
			(start 3.401 -1.011)
			(end 3.401 1.011)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "00045109-5913-4be1-b844-15e0dd7db124")
		)
		(fp_line
			(start 3.361 -1.098)
			(end 3.361 1.098)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3bca68c0-66b5-46e6-8e79-536cd78f75d7")
		)
		(fp_line
			(start 3.321 -1.178)
			(end 3.321 1.178)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "53e256ff-44a7-4057-a9f3-069e9fb5f9b7")
		)
		(fp_line
			(start 3.281 -1.251)
			(end 3.281 1.251)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "45423e9d-d8f5-4422-af97-69492cc653d4")
		)
		(fp_line
			(start 3.241 -1.319)
			(end 3.241 1.319)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dd093b64-824d-4976-b625-b888111948c5")
		)
		(fp_line
			(start 3.201 -1.383)
			(end 3.201 1.383)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6001771f-dc1b-4fb8-b904-f86466307703")
		)
		(fp_line
			(start 3.161 -1.443)
			(end 3.161 1.443)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4bdba487-696c-4c14-b610-eb8445b65261")
		)
		(fp_line
			(start 3.121 -1.5)
			(end 3.121 1.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d3cabff1-b0dc-41af-8a9f-a33abb58a7fb")
		)
		(fp_line
			(start 3.081 -1.554)
			(end 3.081 1.554)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dbd3261d-8c67-4069-be45-b03e93056267")
		)
		(fp_line
			(start 3.041 -1.605)
			(end 3.041 1.605)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bd42b19b-7615-46e1-af96-f04b16cc4e9d")
		)
		(fp_line
			(start 3.001 1.04)
			(end 3.001 1.653)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2b67d6e7-2fc6-49e3-ad54-f212b38f81a7")
		)
		(fp_line
			(start 3.001 -1.653)
			(end 3.001 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "64a031a3-a1ec-4901-b808-b885a44d23e1")
		)
		(fp_line
			(start 2.961 1.04)
			(end 2.961 1.699)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aac2b8a2-27ec-4a74-bf95-ee17a17418bd")
		)
		(fp_line
			(start 2.961 -1.699)
			(end 2.961 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "51dceee2-16f6-43f7-8551-cd3dd85bdcc4")
		)
		(fp_line
			(start 2.921 1.04)
			(end 2.921 1.743)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "12ba1fea-5e54-45bf-b5a9-35290a664022")
		)
		(fp_line
			(start 2.921 -1.743)
			(end 2.921 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7a3422f5-2619-4e48-b9e7-1863cfd39e86")
		)
		(fp_line
			(start 2.881 1.04)
			(end 2.881 1.785)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "42909113-9a61-4f6f-aac9-60c1d8be5c40")
		)
		(fp_line
			(start 2.881 -1.785)
			(end 2.881 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bb2958d7-b3a8-487c-9fe3-9356c393d088")
		)
		(fp_line
			(start 2.841 1.04)
			(end 2.841 1.826)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e604e3d2-7524-4120-afb6-c5ba24ede1d0")
		)
		(fp_line
			(start 2.841 -1.826)
			(end 2.841 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "68283d29-bee9-41c1-9726-d64116b152e2")
		)
		(fp_line
			(start 2.801 1.04)
			(end 2.801 1.864)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d35f4c36-c4c9-4805-8711-793943c96017")
		)
		(fp_line
			(start 2.801 -1.864)
			(end 2.801 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0425fe27-3a5a-484f-8e89-3b29f5c0b252")
		)
		(fp_line
			(start 2.761 1.04)
			(end 2.761 1.901)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "341ffc43-b0d9-4f06-b119-d08a33807afa")
		)
		(fp_line
			(start 2.761 -1.901)
			(end 2.761 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ef92bf29-ade3-44da-af13-b35a702664d2")
		)
		(fp_line
			(start 2.721 1.04)
			(end 2.721 1.937)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1ca44b92-16e0-4e20-a0b4-ad15b6ac9db2")
		)
		(fp_line
			(start 2.721 -1.937)
			(end 2.721 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2efd99b4-49ab-46f6-aca3-80d3ae684b49")
		)
		(fp_line
			(start 2.681 1.04)
			(end 2.681 1.971)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e0b74608-447b-47fc-9ce4-4d5ee504c5ca")
		)
		(fp_line
			(start 2.681 -1.971)
			(end 2.681 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ff287a41-c6c5-4e9b-a891-6fb3628e3f73")
		)
		(fp_line
			(start 2.641 1.04)
			(end 2.641 2.004)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "af9727d6-942f-4544-8b36-390cd2ab52f9")
		)
		(fp_line
			(start 2.641 -2.004)
			(end 2.641 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cdc80964-046c-45ff-b2b0-8eef9a3034cc")
		)
		(fp_line
			(start 2.601 1.04)
			(end 2.601 2.035)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0f4f3b06-a409-4f0b-99e5-e8eda1ee3b46")
		)
		(fp_line
			(start 2.601 -2.035)
			(end 2.601 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a3cd8cd2-8daa-4701-b807-e803f6afbe1f")
		)
		(fp_line
			(start 2.561 1.04)
			(end 2.561 2.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "abf6e0c7-9210-478f-a403-05823b3af8e4")
		)
		(fp_line
			(start 2.561 -2.065)
			(end 2.561 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "eb153a12-1fab-4d00-8e50-40d6a2e44fa9")
		)
		(fp_line
			(start 2.521 1.04)
			(end 2.521 2.095)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5c3d0e22-231c-42b0-93c5-cb380fe9ccf4")
		)
		(fp_line
			(start 2.521 -2.095)
			(end 2.521 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cdb69d78-1587-4324-80ae-182aa748b2e3")
		)
		(fp_line
			(start 2.481 1.04)
			(end 2.481 2.122)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e59afef1-7ed8-4ff7-9d28-9033bd62c9a5")
		)
		(fp_line
			(start 2.481 -2.122)
			(end 2.481 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7efb57f1-db73-4c55-94fc-0787d3393e40")
		)
		(fp_line
			(start 2.441 1.04)
			(end 2.441 2.149)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d2532258-1299-4dbe-93b7-4f90850eef24")
		)
		(fp_line
			(start 2.441 -2.149)
			(end 2.441 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1f8b2fcf-309a-4dc4-bd38-d4a7598b2455")
		)
		(fp_line
			(start 2.401 1.04)
			(end 2.401 2.175)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3239c564-0567-4b20-af3e-9300849e23b7")
		)
		(fp_line
			(start 2.401 -2.175)
			(end 2.401 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ef22b5a4-be54-428b-9883-fccfa02b0373")
		)
		(fp_line
			(start 2.361 1.04)
			(end 2.361 2.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c230ec50-03d2-496f-9278-93951c15a480")
		)
		(fp_line
			(start 2.361 -2.2)
			(end 2.361 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3cb9ca05-e63e-43b6-a08d-6005d052afde")
		)
		(fp_line
			(start 2.321 1.04)
			(end 2.321 2.224)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "45674b93-2093-4726-8505-13bac5b71993")
		)
		(fp_line
			(start 2.321 -2.224)
			(end 2.321 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "400ebd97-77ad-4a58-819a-605878e15f6c")
		)
		(fp_line
			(start 2.281 1.04)
			(end 2.281 2.247)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c04270b8-f42b-4d73-9250-5986898c4969")
		)
		(fp_line
			(start 2.281 -2.247)
			(end 2.281 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "281b5b99-5d5c-4c01-8ba6-d8bd1850ca08")
		)
		(fp_line
			(start 2.241 1.04)
			(end 2.241 2.268)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b532e8d4-e341-4b08-9e03-f33a67eed6ec")
		)
		(fp_line
			(start 2.241 -2.268)
			(end 2.241 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9a89376d-5344-4643-980c-f753b657e194")
		)
		(fp_line
			(start 2.201 1.04)
			(end 2.201 2.29)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e68af796-b0a6-4b1a-bd6b-0176f044096f")
		)
		(fp_line
			(start 2.201 -2.29)
			(end 2.201 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d75f58f8-460c-47a8-b18e-ccd913cbf14e")
		)
		(fp_line
			(start 2.161 1.04)
			(end 2.161 2.31)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c632c28f-28d3-49e7-b4b6-b2a97e8c77ff")
		)
		(fp_line
			(start 2.161 -2.31)
			(end 2.161 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6b96cb84-e7a5-49cf-8dd0-c0ab9de94da3")
		)
		(fp_line
			(start 2.121 1.04)
			(end 2.121 2.329)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8168fa50-b35b-49a6-b565-3970072c5730")
		)
		(fp_line
			(start 2.121 -2.329)
			(end 2.121 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0cf7c30d-4bb6-4abb-b9b4-24887ae11687")
		)
		(fp_line
			(start 2.081 1.04)
			(end 2.081 2.348)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e9578d54-cac0-4402-9289-99a3c18068a6")
		)
		(fp_line
			(start 2.081 -2.348)
			(end 2.081 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c8e0088f-13ec-4729-ba4e-8972d57dae73")
		)
		(fp_line
			(start 2.041 1.04)
			(end 2.041 2.365)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5e377169-b850-45b9-907b-c4d6af70f8c3")
		)
		(fp_line
			(start 2.041 -2.365)
			(end 2.041 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d4508402-fc35-4b89-8e76-024437c1dc11")
		)
		(fp_line
			(start 2.001 1.04)
			(end 2.001 2.382)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ba12f08c-0cce-451c-a747-e0819ec69d5c")
		)
		(fp_line
			(start 2.001 -2.382)
			(end 2.001 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "25b38d64-df50-4e7e-82f5-20341122b250")
		)
		(fp_line
			(start 1.961 1.04)
			(end 1.961 2.398)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e2d0b886-e153-4727-9044-90d78062f78c")
		)
		(fp_line
			(start 1.961 -2.398)
			(end 1.961 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "99a7dad5-bb50-4891-abd4-bf2667dfdd0d")
		)
		(fp_line
			(start 1.921 1.04)
			(end 1.921 2.414)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7b2202cc-4d37-41a2-93b4-4040c550cc61")
		)
		(fp_line
			(start 1.921 -2.414)
			(end 1.921 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c779a177-f708-44d1-9569-4e9b188558c7")
		)
		(fp_line
			(start 1.881 1.04)
			(end 1.881 2.428)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5baaa8a4-9140-4203-9cf9-db16942b0c37")
		)
		(fp_line
			(start 1.881 -2.428)
			(end 1.881 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "09bd29a6-ab02-41a7-b981-483056d68563")
		)
		(fp_line
			(start 1.841 1.04)
			(end 1.841 2.442)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "15a09e37-53e1-474f-9ba7-3a66a7c3ad95")
		)
		(fp_line
			(start 1.841 -2.442)
			(end 1.841 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "07a0d46c-36bd-48f6-b390-f389105ffed5")
		)
		(fp_line
			(start 1.801 1.04)
			(end 1.801 2.455)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ac2a9684-7dd3-4a08-b5f0-d22567e69856")
		)
		(fp_line
			(start 1.801 -2.455)
			(end 1.801 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0084ce6a-f041-44e6-bfd6-91ad533357e7")
		)
		(fp_line
			(start 1.761 1.04)
			(end 1.761 2.468)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e3a29d13-5a5d-4687-8e10-c586de1472bb")
		)
		(fp_line
			(start 1.761 -2.468)
			(end 1.761 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "73a89941-d8ed-4e82-8061-1f851703a432")
		)
		(fp_line
			(start 1.721 1.04)
			(end 1.721 2.48)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5c9b3b5e-e81b-4166-9ad6-18453d699814")
		)
		(fp_line
			(start 1.721 -2.48)
			(end 1.721 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "187f69dd-f08d-432e-89f8-5ac9508b3543")
		)
		(fp_line
			(start 1.68 1.04)
			(end 1.68 2.491)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b0065510-0078-4a2c-abd7-b3ed7591edc6")
		)
		(fp_line
			(start 1.68 -2.491)
			(end 1.68 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f23f6711-5480-4485-ac64-f762e56f94f9")
		)
		(fp_line
			(start 1.64 1.04)
			(end 1.64 2.501)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3b782638-5d7e-4cd6-97c6-a3add5cd077b")
		)
		(fp_line
			(start 1.64 -2.501)
			(end 1.64 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "323572a9-4d5d-4637-af84-6343f4066bea")
		)
		(fp_line
			(start 1.6 1.04)
			(end 1.6 2.511)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4c90da6c-b7bd-4e86-90ca-342b1f26a720")
		)
		(fp_line
			(start 1.6 -2.511)
			(end 1.6 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0c58a059-72a9-4c58-b202-dc72f7e3dedb")
		)
		(fp_line
			(start 1.56 1.04)
			(end 1.56 2.52)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "40f44b82-c538-4510-987f-4689439e0260")
		)
		(fp_line
			(start 1.56 -2.52)
			(end 1.56 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "449f8fa0-fdab-4031-b407-7db6353476a9")
		)
		(fp_line
			(start 1.52 1.04)
			(end 1.52 2.528)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "506f8f75-8ec6-4c6b-bea6-3572eb4fc60e")
		)
		(fp_line
			(start 1.52 -2.528)
			(end 1.52 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4ff1960c-4bb4-4a33-ba2e-ad58f7491a00")
		)
		(fp_line
			(start 1.48 1.04)
			(end 1.48 2.536)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "028a7825-c952-41b7-af94-6c8a6a97bce7")
		)
		(fp_line
			(start 1.48 -2.536)
			(end 1.48 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ff4fc111-71ee-4665-ae09-f499820c32f1")
		)
		(fp_line
			(start 1.44 1.04)
			(end 1.44 2.543)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8ac3d2fd-84f9-4942-beee-1252007851d1")
		)
		(fp_line
			(start 1.44 -2.543)
			(end 1.44 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9cb0a480-f3bd-44bf-a872-c88b10b0bff1")
		)
		(fp_line
			(start 1.4 1.04)
			(end 1.4 2.55)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e5e01b6a-68ea-4934-a066-a17cd75c39e3")
		)
		(fp_line
			(start 1.4 -2.55)
			(end 1.4 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d8c5da78-938f-4c10-a479-dff59f1eae00")
		)
		(fp_line
			(start 1.36 1.04)
			(end 1.36 2.556)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f302143a-7922-4e35-86a2-b47ab0ecde3a")
		)
		(fp_line
			(start 1.36 -2.556)
			(end 1.36 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9ed279bf-c711-4158-add5-eedab2815ae0")
		)
		(fp_line
			(start 1.32 1.04)
			(end 1.32 2.561)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "72d5f5b2-ca29-438a-83fa-a3835f4165e4")
		)
		(fp_line
			(start 1.32 -2.561)
			(end 1.32 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e8cea380-ffbc-44ac-a194-ad3002c368f0")
		)
		(fp_line
			(start 1.28 1.04)
			(end 1.28 2.565)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "da7dd396-4df2-44f8-89eb-641e82467d6b")
		)
		(fp_line
			(start 1.28 -2.565)
			(end 1.28 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "546cb8c5-fbf2-418a-9d41-5e5f46437570")
		)
		(fp_line
			(start 1.24 1.04)
			(end 1.24 2.569)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9241b629-cda3-4444-80ab-3b4bff7b6a17")
		)
		(fp_line
			(start 1.24 -2.569)
			(end 1.24 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "adf336e9-1459-43c2-9500-798afa528cd2")
		)
		(fp_line
			(start 1.2 1.04)
			(end 1.2 2.573)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e2a8c90b-a3de-43c5-a62c-71f0aff80413")
		)
		(fp_line
			(start 1.2 -2.573)
			(end 1.2 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "008d874b-273d-4017-ba7e-8ed3d768505e")
		)
		(fp_line
			(start 1.16 1.04)
			(end 1.16 2.576)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f715b309-2634-409d-8eef-4ae090926e0c")
		)
		(fp_line
			(start 1.16 -2.576)
			(end 1.16 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c4eb82bc-9229-465c-b827-96257abf7059")
		)
		(fp_line
			(start 1.12 1.04)
			(end 1.12 2.578)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ea3da1a0-b9c3-4c23-9b38-b76c16ff2089")
		)
		(fp_line
			(start 1.12 -2.578)
			(end 1.12 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dc14871d-54df-4467-ad42-b036625be885")
		)
		(fp_line
			(start 1.08 1.04)
			(end 1.08 2.579)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4366c510-5315-4e49-b656-d94f1658d8d8")
		)
		(fp_line
			(start 1.08 -2.579)
			(end 1.08 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "50e5e06a-acf4-4b16-8ae7-a5cd4c9c4d32")
		)
		(fp_line
			(start 1.04 1.04)
			(end 1.04 2.58)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "66834141-c3a7-4e6b-a26e-f014a29d4b2b")
		)
		(fp_line
			(start 1.04 -2.58)
			(end 1.04 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e517255b-d7d7-4330-9866-3ef6f232e228")
		)
		(fp_line
			(start 1 1.04)
			(end 1 2.58)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "47426242-51e0-4d1a-aa09-aacbeab3c426")
		)
		(fp_line
			(start 1 -2.58)
			(end 1 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d3491b06-512a-48a0-8c07-2e983225a79c")
		)
		(fp_line
			(start -1.554775 -1.725)
			(end -1.554775 -1.225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f30ec4b1-7594-4bba-a2c1-fb55842fa33c")
		)
		(fp_line
			(start -1.804775 -1.475)
			(end -1.304775 -1.475)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "80be06c8-8930-442c-b422-f34d19daf8a7")
		)
		(fp_circle
			(center 1 0)
			(end 3.62 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "7eddfe58-74b4-491a-889e-d1cbbe407bc2")
		)
		(fp_circle
			(center 1 0)
			(end 3.75 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill none)
			(layer "F.CrtYd")
			(uuid "0e370603-96f6-40b3-8a8c-87f13be52e16")
		)
		(fp_line
			(start -0.883605 -1.3375)
			(end -0.883605 -0.8375)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e9e08ce3-f979-4db7-a01f-1a941f544c8a")
		)
		(fp_line
			(start -1.133605 -1.0875)
			(end -0.633605 -1.0875)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "22a1a4f3-ca80-438b-b45f-3678536584b8")
		)
		(fp_circle
			(center 1 0)
			(end 3.5 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "23b53cc8-b631-455a-ad1f-72c78675abfd")
		)
		(fp_text user "${REFERENCE}"
			(at 1 0 360)
			(layer "F.Fab")
			(uuid "94bfdf0f-d240-4139-b50a-b9a6d6c0394b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
			(uuid "e26a36e0-7241-4390-8f94-78223ed2b022")
		)
		(pad "2" thru_hole circle
			(at 2 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J2-Pin_1)")
			(pintype "passive")
			(uuid "e98487cc-3568-4473-924c-ee2dd8caf83f")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-8_W7.62mm"
		(layer "F.Cu")
		(uuid "2fa7f398-fe07-4414-8e2c-675eeae49fff")
		(at 98.2 97.7)
		(descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U2"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
			(uuid "44d29630-7346-4acd-bd97-f819e71b7a64")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "ATtiny45-20P"
			(at 3.81 9.95 0)
			(layer "F.Fab")
			(uuid "6c95fe55-4cf7-4428-b109-f8e6de595b2a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b471123a-f704-4078-942c-1c6d72220125")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "dde6d63a-4fa2-4f05-92bc-746faf2f097d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 256B EEPROM, debugWIRE, DIP-8"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d5ebc88d-39e5-445b-ba4d-d94047637c82")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/cc4e7474-c0ce-4289-b3c6-7af942381fa0")
		(sheetfile "led-controller.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 8.95)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "52f59e6d-c541-4963-b417-43d69eebae06")
		)
		(fp_line
			(start 1.16 8.95)
			(end 6.46 8.95)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "de95a92c-fd1a-4e45-b550-71c4d4779d0e")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "09985e62-ae77-4013-92d3-5d2ffca627e4")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ff87dc49-f822-4ac6-8d2d-48bfa6c9b043")
		)
		(fp_line
			(start 6.46 8.95)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "87efbe7f-2538-43a8-bdf7-33dfc540c1fa")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fa9f8e55-4a18-42ad-b873-15bbfde94964")
		)
		(fp_line
			(start -1.1 -1.55)
			(end -1.1 9.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0030d3f3-6137-4a69-9b78-30f466e8f267")
		)
		(fp_line
			(start -1.1 9.15)
			(end 8.7 9.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6ce6902a-d33e-4579-8189-2c64864d7e34")
		)
		(fp_line
			(start 8.7 -1.55)
			(end -1.1 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "810019c3-4c99-4557-b518-082c863216a1")
		)
		(fp_line
			(start 8.7 9.15)
			(end 8.7 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b821d929-eb7f-4a6a-8349-621249a75a92")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "20317ac1-109d-400d-ae2e-48f863f0debb")
		)
		(fp_line
			(start 0.635 8.89)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6528ec21-4a1c-4f07-8c74-14ac01716126")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5e9d6178-fd16-418e-9db7-cf49b80d5268")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 8.89)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8ca0e3ba-d55f-4ea2-83be-2a387d7c9bda")
		)
		(fp_line
			(start 6.985 8.89)
			(end 0.635 8.89)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "63ac5c11-e6b0-450f-bfd8-1ce146a9a5c4")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 3.81 0)
			(layer "F.Fab")
			(uuid "f375b874-738c-41cc-a9d2-0f02b4a056c9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(J2-Pin_6)")
			(pinfunction "~{RESET}/PB5")
			(pintype "bidirectional")
			(uuid "38b2bd54-dc51-485c-a741-12bb0120a139")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "unconnected-(U2-XTAL1{slash}PB3-Pad2)")
			(pinfunction "XTAL1/PB3")
			(pintype "bidirectional")
			(uuid "6227f91b-47dd-4b65-9d73-01dd386037fe")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(Q3-G)")
			(pinfunction "XTAL2/PB4")
			(pintype "bidirectional")
			(uuid "013a1319-7eba-429e-bff0-059051449343")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "f5aeb55a-8501-49ae-96b3-68f040dafc7c")
		)
		(pad "5" thru_hole oval
			(at 7.62 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(J2-Pin_3)")
			(pinfunction "AREF/PB0")
			(pintype "bidirectional")
			(uuid "09e38363-b5a7-4b78-86af-f8d2e39aa523")
		)
		(pad "6" thru_hole oval
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J2-Pin_4)")
			(pinfunction "PB1")
			(pintype "bidirectional")
			(uuid "f92c4cc9-5fe4-4f3f-966c-30718f7a4817")
		)
		(pad "7" thru_hole oval
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(J2-Pin_5)")
			(pinfunction "PB2")
			(pintype "bidirectional")
			(uuid "5943af82-cbd3-48eb-80e4-63a71ae21988")
		)
		(pad "8" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J2-Pin_1)")
			(pinfunction "VCC")
			(pintype "power_in")
			(uuid "00f82f41-47e0-4fac-b921-82cdf9461821")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Vertical"
		(layer "F.Cu")
		(uuid "45f1578e-d440-49f2-a2d3-cb9fd12dcad7")
		(at 114.42 96.5)
		(descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Vertical RM 2.54mm")
		(property "Reference" "U1"
			(at 2.54 -4.27 0)
			(layer "F.SilkS")
			(uuid "a5f492a0-ed63-44d6-9ac2-e3a6600fe376")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LM7805_TO220"
			(at 2.54 2.5 0)
			(layer "F.Fab")
			(uuid "540a4e4d-a3a1-48ce-a38b-762446b99d3e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "255769bd-3513-490c-8f83-2cf8cbe1901e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e89acf2b-bde0-435e-ba7a-0d26e158cd26")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Positive 1A 35V Linear Regulator, Fixed Output 5V, TO-220"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "80b56d12-52ea-4f00-816f-9d3a13ad0062")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/14118208-d22c-401e-82d3-6e7cea3c6576")
		(sheetfile "led-controller.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.58 -3.27)
			(end -2.58 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f6c9ed42-b26a-4f70-bae5-3ac972fe815d")
		)
		(fp_line
			(start -2.58 -3.27)
			(end 7.66 -3.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8fac2ff0-e19f-476c-96cc-1bdd20da5173")
		)
		(fp_line
			(start -2.58 -1.76)
			(end 7.66 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "97e7b4b9-891c-41bb-a2a5-d91e82b51a17")
		)
		(fp_line
			(start -2.58 1.371)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2ea99d03-4560-45f9-8f6c-aa971c2bd07a")
		)
		(fp_line
			(start 0.69 -3.27)
			(end 0.69 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fbd61989-75f3-4dd9-9399-0d26b997b362")
		)
		(fp_line
			(start 4.391 -3.27)
			(end 4.391 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cad53296-257b-4ae5-984d-57715e8e836f")
		)
		(fp_line
			(start 7.66 -3.27)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "42c7be10-0651-40ab-b68a-0bf385a57e25")
		)
		(fp_line
			(start -2.71 -3.4)
			(end -2.71 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fa043b65-a50b-4ecc-beff-847e1ecf78c3")
		)
		(fp_line
			(start -2.71 1.51)
			(end 7.79 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2e6acc0d-ebec-499d-97f9-b51b8b63ba95")
		)
		(fp_line
			(start 7.79 -3.4)
			(end -2.71 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "38f2f3c7-d095-472c-b1ce-75e3eb171600")
		)
		(fp_line
			(start 7.79 1.51)
			(end 7.79 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "472bb8b7-3142-4350-9812-71c8b2ddf794")
		)
		(fp_line
			(start -2.46 -3.15)
			(end -2.46 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "af13cfda-9036-41ce-9f84-e3858a72feda")
		)
		(fp_line
			(start -2.46 -1.88)
			(end 7.54 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6dd90304-f348-45f8-a67f-fd264fceb01d")
		)
		(fp_line
			(start -2.46 1.25)
			(end 7.54 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e4d143be-e86f-43b2-9be0-7fbeecb72cd4")
		)
		(fp_line
			(start 0.69 -3.15)
			(end 0.69 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2e6b6829-51ba-4d78-8540-231819afca6b")
		)
		(fp_line
			(start 4.39 -3.15)
			(end 4.39 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1c4ee764-d255-4cbc-8996-d485032b7648")
		)
		(fp_line
			(start 7.54 -3.15)
			(end -2.46 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f7a374ae-bd1d-4efa-967f-5404dcfd6b8a")
		)
		(fp_line
			(start 7.54 1.25)
			(end 7.54 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0e87e472-5f9c-4f95-bd88-7c9dca880d9c")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 -4.27 0)
			(layer "F.Fab")
			(uuid "fcc6ed32-b356-488a-b5c9-f8407c80038a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(BT1-+)")
			(pinfunction "VI")
			(pintype "power_in")
			(uuid "b211dc9b-ffdd-4364-930e-17ef62a1eb5a")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "f48d6512-ca96-4e0d-8b66-6cde645af0fb")
		)
		(pad "3" thru_hole oval
			(at 5.08 0)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J2-Pin_1)")
			(pinfunction "VO")
			(pintype "power_out")
			(uuid "7b4b4a85-0bb3-420d-93c7-e76f89a3ce84")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "638b682d-0078-46b1-8a79-66609c2b5eef")
		(at 99 93.675 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 0 -1.43 -90)
			(layer "F.SilkS")
			(uuid "7bdb11a2-8409-4970-b890-1e9cc0869182")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100k"
			(at 0 1.43 -90)
			(layer "F.Fab")
			(uuid "f81afd17-fb74-4d67-a050-b0549adf7e5c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "094131a9-53b0-463a-9c4f-8294602c0e44")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "76390bcf-be2a-4521-9d58-e0946296bcd9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ef3fa10c-7440-40c9-ab20-f0c4e54bc491")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Feld4" ""
			(at -20.32 172.72 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "cfff765e-f793-404c-a3f7-8388a92cca1f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/304b0b82-58bd-438d-a5d7-69c727691bf3")
		(sheetfile "led-controller.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "97a24403-2229-40c6-8f9f-ab4cad8709cd")
		)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9248b1b8-3e48-4c0e-b6c8-4f58998a0bac")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0e6e7d53-ca59-4a6b-81cb-711fd7afc2a7")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "10437692-f689-453f-bee2-2f568dd3fbec")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b2316fd0-69e7-455c-9746-9766759220fd")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "019d7275-c4e6-4f14-9616-350bc70c0bc0")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "999cf2ca-28a8-416b-9134-9559b07f8dc6")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bb8672e0-5ae2-4522-9f32-11178b7c5b6a")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "008c66e8-52b7-450f-a7b3-d16ecb5c6da6")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "da9db077-7d2d-4bc5-80ba-3a8de0bd69c0")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
			(uuid "6aa72ea6-379c-4659-9cea-8cd4c01b99d8")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "Net-(Q3-G)")
			(pintype "passive")
			(uuid "dd5a795a-f211-4e33-8ba8-b062b6d37549")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
			(uuid "5a405639-1228-4670-ba8a-90aa3119947a")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical"
		(layer "F.Cu")
		(uuid "65685b0a-7661-4dc8-ba35-8b438ab8f725")
		(at 122.35 106 -90)
		(descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x06 2.54mm single row")
		(property "Reference" "J2"
			(at 0 -2.33 90)
			(layer "F.SilkS")
			(uuid "14eb4dde-e85d-4bb0-8cd2-5f4185549e41")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x06_Socket"
			(at 0 15.03 90)
			(layer "F.Fab")
			(uuid "f71435fb-4f52-4a43-82c8-8b821cdbfef3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "b9cbe08d-56fa-40b8-befb-44b3c73b5986")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "66fc815f-aaf0-4885-a5bb-6f45356b880d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x06, script generated"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "8de24189-0c1a-42dc-a232-27e3f96cf3c3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/ccc2476a-3d91-4d08-9b99-901f9f21b284")
		(sheetfile "led-controller.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.33 14.03)
			(end 1.33 14.03)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0586aaa7-acf7-498e-a47d-4c259cd246fc")
		)
		(fp_line
			(start -1.33 1.27)
			(end -1.33 14.03)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "69e1d444-27eb-4a6e-b4a5-46cd513ec877")
		)
		(fp_line
			(start -1.33 1.27)
			(end 1.33 1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b67aaac7-090c-4c78-87c0-aa05c7208943")
		)
		(fp_line
			(start 1.33 1.27)
			(end 1.33 14.03)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2ce916a0-84f4-41c1-9b10-c29b2232da4e")
		)
		(fp_line
			(start -1.33 0)
			(end -1.33 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2bab00c6-60a1-465a-a1e9-37ebc510eb6e")
		)
		(fp_line
			(start -1.33 -1.33)
			(end 0 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "84768567-8dc3-4832-a431-521eafb205f6")
		)
		(fp_line
			(start -1.8 14.5)
			(end 1.8 14.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5e47e16b-9fe9-4818-89f0-4cd741f65ebe")
		)
		(fp_line
			(start 1.8 14.5)
			(end 1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "63980e53-273f-4f13-82ce-79feb438e7cd")
		)
		(fp_line
			(start -1.8 -1.8)
			(end -1.8 14.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "964ee3ed-dc2d-4bbc-a6c7-5dc71df657df")
		)
		(fp_line
			(start 1.8 -1.8)
			(end -1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1ca619cc-548c-43ac-a03b-1c80141076e4")
		)
		(fp_line
			(start -1.27 13.97)
			(end -1.27 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "29cda9f4-8fd7-4cf6-99df-d85e57ba6257")
		)
		(fp_line
			(start 1.27 13.97)
			(end -1.27 13.97)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4279678d-ddb7-4241-9a6c-62e882a1e63c")
		)
		(fp_line
			(start -1.27 -0.635)
			(end -0.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "14ad99dd-0e63-4054-b5f8-f80955eb90eb")
		)
		(fp_line
			(start -0.635 -1.27)
			(end 1.27 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cadc6efe-2d78-4569-9941-06d09d317164")
		)
		(fp_line
			(start 1.27 -1.27)
			(end 1.27 13.97)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d639c25a-eda4-4e7e-91f1-dbe91f701a86")
		)
		(fp_text user "${REFERENCE}"
			(at 0 6.35 360)
			(layer "F.Fab")
			(uuid "12cd8979-6bc8-4c8d-831a-d6d4b8163510")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J2-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "f62d68b3-fa49-4e12-9ba6-51c3a0288d3b")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "d8d10b97-e5bc-4122-86e8-29beef3a6afe")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(J2-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "fdd2187d-3779-45bb-83a1-ccb0c046f645")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J2-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
			(uuid "7a658cc9-eb9c-494a-a05e-4de7da545789")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(J2-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
			(uuid "aa004b1a-9d45-4c6b-a669-375cc3205760")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(J2-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
			(uuid "7fb76073-1fbb-4627-8c53-b08fbde8bf88")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "6e9df83c-66b6-423e-b0fc-288e573f8571")
		(at 104 93.675 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 -1.43 -90)
			(layer "F.SilkS")
			(uuid "a9711b83-2e54-461d-825c-94eddb8c5753")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100k"
			(at 0 1.43 -90)
			(layer "F.Fab")
			(uuid "30a3f70e-bd19-4c5e-99ce-e6fa03c4681b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c0ba32a0-0dd1-4fff-bf79-dc95370a5bf6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "67348cb4-95db-410c-abf3-c3cef064d2c9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "80be614a-3b70-47c6-bf3d-3a5878985d3d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/267fb370-609d-4c7e-8bd4-8b6ac6591673")
		(sheetfile "led-controller.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e5a1f863-4712-4252-8e7a-e3c55f5468b0")
		)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4253d0ba-9ad7-4881-be96-59bc809b5a36")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1afc3335-bc4f-404a-b388-948946d04bf8")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "768d5cd8-b8c4-4c61-8a5c-6592e5daaae8")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "347708d6-c6fe-4786-a0c5-fb89d7eaa79f")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b03acc72-e126-48a1-b6fa-4e4a763c9025")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0b8cb34e-71c4-47e2-83ff-f92e02019b94")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bdb562dd-3397-4d90-840c-d2d91c03d86a")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "80efb320-96e8-4702-829b-2ef5b6151b1a")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2c464b52-9cfe-4ca9-9419-c5e8f5c20e89")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
			(uuid "9688cb83-02fb-456c-9d5d-949b87147b47")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "Net-(J2-Pin_4)")
			(pintype "passive")
			(uuid "ca664df1-7e9c-4673-b4d6-55930dd69fc1")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
			(uuid "2e21af05-bd91-49b6-a96a-9aca2b968104")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(uuid "7401d5f0-600f-4d6b-87a1-6982f58d4696")
		(at 108.5 93.675 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 -1.43 -90)
			(layer "F.SilkS")
			(uuid "223802f5-300e-4523-aa40-36ce9c9aedaa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100k"
			(at 0 1.43 -90)
			(layer "F.Fab")
			(uuid "4ad8a8ed-327a-40bf-bbd7-ffab0a8f7224")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fdcee84d-d7cd-4d2d-b291-1bd478e6598d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5efc78a9-fbba-4c87-8b07-36eb62cb8541")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9c022ccf-cc44-4e7b-be15-c9fb4b5eb1cd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/90dbdc91-46c9-4b01-b3fc-3a001184cea4")
		(sheetfile "led-controller.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.237258 0.5225)
			(end 0.237258 0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b4988063-b07b-42d0-8331-ee77d3c0e50a")
		)
		(fp_line
			(start -0.237258 -0.5225)
			(end 0.237258 -0.5225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "beb94fe6-9e2d-4152-896b-6be6a88e4ea4")
		)
		(fp_line
			(start -1.48 0.73)
			(end -1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8e8a6df0-9f20-47f8-9f62-e2932fec61f6")
		)
		(fp_line
			(start 1.48 0.73)
			(end -1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c3ee645c-5e23-4fc8-a759-e17735a914c4")
		)
		(fp_line
			(start -1.48 -0.73)
			(end 1.48 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c54f5f8f-8e67-47df-98c5-03219305f73e")
		)
		(fp_line
			(start 1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "89661697-7251-43f0-82e6-ae624e8a2774")
		)
		(fp_line
			(start -0.8 0.4125)
			(end -0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "647a9bf6-75dd-4556-a34f-4680a28c79e3")
		)
		(fp_line
			(start 0.8 0.4125)
			(end -0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aece362c-d924-437a-898b-b0fc14f37bef")
		)
		(fp_line
			(start -0.8 -0.4125)
			(end 0.8 -0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1fa49017-888e-42cd-a49e-0a0855a75202")
		)
		(fp_line
			(start 0.8 -0.4125)
			(end 0.8 0.4125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "363892f0-b1d1-4b6c-8432-5512bf44330b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
			(uuid "a9d44e07-d129-4237-9988-dbf26b11352e")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "Net-(J2-Pin_3)")
			(pintype "passive")
			(uuid "b71b4965-4a2f-4700-a20b-64b968c3c926")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
			(uuid "34a3fdd3-275c-4460-b46f-a2f60ecf6018")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_TE-Connectivity:TerminalBlock_TE_282834-4_1x04_P2.54mm_Horizontal"
		(layer "F.Cu")
		(uuid "75756c00-b1b8-4f63-b710-e816d1bf05f1")
		(at 109.815 83 180)
		(descr "Terminal Block TE 282834-4, 4 pins, pitch 2.54mm, size 10.620000000000001x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity")
		(tags "THT Terminal Block TE 282834-4 pitch 2.54mm size 10.620000000000001x6.5mm^2 drill 1.1mm pad 2.1mm")
		(property "Reference" "J1"
			(at 3.81 -4.37 360)
			(layer "F.SilkS")
			(uuid "04d07af4-5601-4c6f-b68f-e5d5c88079e8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "+12V_STRIP"
			(at 3.81 4.37 360)
			(layer "F.Fab")
			(uuid "e5c16a1b-ea3f-4509-a638-94233ebed63f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
			(uuid "501e0726-0002-46b1-98cb-aeaf978aa890")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
			(uuid "e1f74a3c-c700-447c-be02-9a73c597782e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
			(uuid "993b82b1-6f1a-47fe-9b62-c17487246810")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/69d099f9-9098-463f-8369-284ce5d555c2")
		(sheetfile "led-controller.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 9.241 -3.37)
			(end 9.241 3.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bdbfa24b-374a-4f06-8d01-2e195cb80ae3")
		)
		(fp_line
			(start -1.62 3.37)
			(end 9.241 3.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "553163c6-fe63-4fca-9627-5b21e6406070")
		)
		(fp_line
			(start -1.62 2.85)
			(end 9.241 2.85)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "93c6920a-8c08-42e8-9136-757fbf9e39d0")
		)
		(fp_line
			(start -1.62 -2.25)
			(end 9.241 -2.25)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1dcf7136-169c-4c9d-a4f4-28dfa1a63664")
		)
		(fp_line
			(start -1.62 -3.37)
			(end 9.241 -3.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5f512801-e1bd-4731-a5a6-ad37a0f0649f")
		)
		(fp_line
			(start -1.62 -3.37)
			(end -1.62 3.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8d9d7547-02be-4605-b29a-1e4a3bbf44a7")
		)
		(fp_line
			(start -1.86 3.61)
			(end -1.46 3.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8efb09f5-d7ba-4b6f-86ea-22c70ee9c2d6")
		)
		(fp_line
			(start -1.86 2.97)
			(end -1.86 3.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e6177ff1-cac3-4253-9af2-e1ada2ef98d3")
		)
		(fp_line
			(start 9.63 3.75)
			(end 9.63 -3.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "44c7da23-8e17-4f21-918c-3e791d311975")
		)
		(fp_line
			(start 9.63 -3.75)
			(end -2 -3.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e250cff0-c70a-432b-a727-8168449a32aa")
		)
		(fp_line
			(start -2 3.75)
			(end 9.63 3.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9fb13903-a5b9-4b6e-b611-cb0f61eb8a5f")
		)
		(fp_line
			(start -2 -3.75)
			(end -2 3.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5a6877e0-70c9-4d8a-b117-9e23908005e7")
		)
		(fp_line
			(start 9.12 3.25)
			(end -1.1 3.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9f5f0d61-3a3a-4279-9a47-04b58c6d134c")
		)
		(fp_line
			(start 9.12 -3.25)
			(end 9.12 3.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ea394ef1-3fca-4a2d-b8ff-75979bbabe0a")
		)
		(fp_line
			(start 8.455 -0.7)
			(end 6.92 0.835)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3a2133f5-90fa-4195-bbf5-c406d230044e")
		)
		(fp_line
			(start 8.321 -0.835)
			(end 6.786 0.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "02b4955d-86e5-48cd-8a7a-c7a8a29cf095")
		)
		(fp_line
			(start 5.915 -0.7)
			(end 4.38 0.835)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "56b9d0e5-cf70-460c-9e9b-d4c5ca59aca5")
		)
		(fp_line
			(start 5.781 -0.835)
			(end 4.246 0.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "46964d96-d042-4ed2-a102-a46fd7acf666")
		)
		(fp_line
			(start 3.375 -0.7)
			(end 1.84 0.835)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "37102ecb-89ac-4ccc-8f51-64e43466881c")
		)
		(fp_line
			(start 3.241 -0.835)
			(end 1.706 0.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4c5a39ed-be69-4b14-9cdb-a69a0f74e304")
		)
		(fp_line
			(start 0.835 -0.7)
			(end -0.701 0.835)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "210ce43c-8cc0-40c7-9eab-4926271f9ec3")
		)
		(fp_line
			(start 0.701 -0.835)
			(end -0.835 0.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0a81756d-0d48-4237-9b45-de9457de96fd")
		)
		(fp_line
			(start -1.1 3.25)
			(end -1.5 2.85)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "664ffd06-76bf-4a02-a565-07979e3ca01e")
		)
		(fp_line
			(start -1.5 2.85)
			(end 9.12 2.85)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8a8f8b1f-a42c-41a2-8280-1d7cfc60f7fb")
		)
		(fp_line
			(start -1.5 2.85)
			(end -1.5 -3.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4e8d446c-ae94-40ae-906a-9ed60e158fa2")
		)
		(fp_line
			(start -1.5 -2.25)
			(end 9.12 -2.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9fb6cd6c-366e-4532-ae19-4a881f6894c2")
		)
		(fp_line
			(start -1.5 -3.25)
			(end 9.12 -3.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2f3d0271-1792-4fd8-8301-bfe83cfe24bd")
		)
		(fp_circle
			(center 7.62 0)
			(end 8.72 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "123f43d6-af62-4ec8-ae9b-f28786bdb624")
		)
		(fp_circle
			(center 5.08 0)
			(end 6.18 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "0808c8cf-b8c5-4044-9143-1925fcdf13d9")
		)
		(fp_circle
			(center 2.54 0)
			(end 3.64 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "78e17422-4c09-4d12-9b93-455f64e68f5e")
		)
		(fp_circle
			(center 0 0)
			(end 1.1 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "244153ba-cecd-45eb-ba6b-069c02eb3f10")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 2 360)
			(layer "F.Fab")
			(uuid "a414f91e-87b3-403f-ba3b-6a00e4b2d5a7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 2.1 2.1)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(BT1-+)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "66eb89f9-da83-4b9a-9398-4584b5ee04fc")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 180)
			(size 2.1 2.1)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(J1-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "6b17ebd4-33f0-4597-9859-ffc2a66d99b6")
		)
		(pad "3" thru_hole circle
			(at 5.08 0 180)
			(size 2.1 2.1)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(J1-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "9e7a878e-f1ab-4c06-bca7-3762377feefa")
		)
		(pad "4" thru_hole circle
			(at 7.62 0 180)
			(size 2.1 2.1)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(J1-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
			(uuid "54f74844-f2b6-411d-a7d6-db4e255320a3")
		)
		(model "${KICAD6_3DMODEL_DIR}/TerminalBlock_TE-Connectivity.3dshapes/TerminalBlock_TE_282834-4_1x04_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock:TerminalBlock_Altech_AK300-2_P5.00mm"
		(layer "F.Cu")
		(uuid "9c632806-6b46-4978-b397-2e9c2514b0b9")
		(at 115 85.5)
		(descr "Altech AK300 terminal block, pitch 5.0mm, 45 degree angled, see http://www.mouser.com/ds/2/16/PCBMETRC-24178.pdf")
		(tags "Altech AK300 terminal block pitch 5.0mm")
		(property "Reference" "BT1"
			(at -1.92 -6.99 0)
			(layer "F.SilkS")
			(uuid "34c29f91-98b7-4e98-822d-45fc875a4367")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "B12V"
			(at 2.78 7.75 0)
			(layer "F.Fab")
			(uuid "a958c20f-0e14-44a8-8ba5-99fdd11894dc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "847f10c8-54e1-494a-8cea-c46ccd4a77b1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "fa59d166-3a83-4f62-9418-17893113e1d0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Multiple-cell battery"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e08f1928-f507-457e-bc4d-fc8fadd4dfba")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/dda22bd2-68a2-4e19-bd3c-f7e3c075b9ca")
		(sheetfile "led-controller.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.65 -6.3)
			(end -2.65 6.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6ed5c804-614e-456c-b86b-c8ba98c35102")
		)
		(fp_line
			(start -2.65 6.3)
			(end 7.7 6.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "50fa9160-edba-4dc4-90b7-b4c4af94716a")
		)
		(fp_line
			(start 7.7 -1.5)
			(end 8.2 -1.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ad3ea20a-9682-43d8-9693-ca0eac5d268a")
		)
		(fp_line
			(start 7.7 3.9)
			(end 7.7 -1.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7cb3ec8e-d2b9-429b-a035-ef968897d5af")
		)
		(fp_line
			(start 7.7 5.35)
			(end 8.2 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "817a0e4f-e446-4ff6-82a8-56abc5cf5b57")
		)
		(fp_line
			(start 7.7 6.3)
			(end 7.7 5.35)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0ad6b5b2-53da-4934-9b6f-352f53befaa4")
		)
		(fp_line
			(start 8.2 -6.3)
			(end -2.65 -6.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "598ece30-116a-48f6-bc85-e76ecbf88167")
		)
		(fp_line
			(start 8.2 -1.2)
			(end 8.2 -6.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a55f4ba0-0574-45dc-af40-73d8d1848999")
		)
		(fp_line
			(start 8.2 3.65)
			(end 7.7 3.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3d659603-d033-4b11-8e45-4088330defd6")
		)
		(fp_line
			(start 8.2 3.7)
			(end 8.2 3.65)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "baae968f-ece0-412f-802c-b571009b23b9")
		)
		(fp_line
			(start 8.2 5.6)
			(end 8.2 3.7)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b8249b7b-8fb5-4c03-9e8e-cccca072e709")
		)
		(fp_line
			(start -2.83 -6.47)
			(end -2.83 6.47)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4862a369-4adc-4e39-bf71-9e8b4348abd6")
		)
		(fp_line
			(start -2.83 -6.47)
			(end 8.36 -6.47)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cfd132da-799e-44a8-84b4-01a0e016b942")
		)
		(fp_line
			(start 8.36 6.47)
			(end -2.83 6.47)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a7763f26-ce7b-48c3-84af-0728a6a7f655")
		)
		(fp_line
			(start 8.36 6.47)
			(end 8.36 -6.47)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "477cfc9f-9a85-4367-bc44-2d6594b9c793")
		)
		(fp_line
			(start -2.58 -3.17)
			(end -2.58 -6.22)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8371740e-e0ca-4a30-8564-d7ae08b1854a")
		)
		(fp_line
			(start -2.58 -3.17)
			(end 7.61 -3.17)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c1c308b5-2c28-454e-bc54-03ad430c7385")
		)
		(fp_line
			(start -2.58 -0.64)
			(end -2.58 -3.17)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4e298545-76ef-4275-9e3b-91c41b5a7275")
		)
		(fp_line
			(start -2.58 -0.64)
			(end -1.64 -0.64)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9f3adb04-eef4-4a68-8339-ed152316894f")
		)
		(fp_line
			(start -2.58 6.22)
			(end -2.58 -0.64)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8793f106-e29d-4be8-9780-3d4847503621")
		)
		(fp_line
			(start -2.58 6.22)
			(end -2.02 6.22)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7b5cadb2-276a-407b-879d-a1a3cc3eb846")
		)
		(fp_line
			(start -2.02 -3.43)
			(end -2.02 -5.97)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5037c137-38e0-4870-bb55-4404346a4d21")
		)
		(fp_line
			(start -2.02 -0.25)
			(end -2.02 4.32)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e71e513c-f6f8-4ae8-a576-248a246b4e4d")
		)
		(fp_line
			(start -2.02 -0.25)
			(end -1.64 -0.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f841a6a8-4adb-4ce0-8ab4-4a204a795559")
		)
		(fp_line
			(start -2.02 4.32)
			(end -2.02 6.22)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "89f48848-70b7-4583-b756-8c6d51825721")
		)
		(fp_line
			(start -2.02 6.22)
			(end 2.04 6.22)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c05a7ad4-59e5-4726-8592-4016df436ff8")
		)
		(fp_line
			(start -1.64 -0.64)
			(end 1.66 -0.64)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fd21c457-80ef-4f84-b099-3adeeed0a834")
		)
		(fp_line
			(start -1.64 0.51)
			(end -1.26 0.51)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "90d4dc73-b1a0-44f8-b6d2-500d1151e59a")
		)
		(fp_line
			(start -1.64 3.68)
			(end -1.64 0.51)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d54e7ccf-2a61-4cd7-a27d-28b837314489")
		)
		(fp_line
			(start -1.62 -4.45)
			(end 1.44 -5.08)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6d6a85a8-d4c3-428b-8ba6-b742d92ada71")
		)
		(fp_line
			(start -1.49 -4.32)
			(end 1.56 -4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bcee40a5-c6c4-4d38-8dc2-213aa5cb2717")
		)
		(fp_line
			(start -1.26 -0.25)
			(end 1.28 -0.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3d5f6938-53b1-4b36-b106-35698d5e2ffe")
		)
		(fp_line
			(start -1.26 2.54)
			(end -1.26 -0.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "367427f5-f1e6-46bb-a0bd-1e2ec7af0ef1")
		)
		(fp_line
			(start -1.26 2.54)
			(end 1.28 2.54)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0b160ac8-2a02-4106-933c-821bdadc4d5a")
		)
		(fp_line
			(start 1.28 2.54)
			(end 1.28 -0.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fbac7cb0-298f-4452-91cf-259b766e95cd")
		)
		(fp_line
			(start 1.66 -0.64)
			(end 3.36 -0.64)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e9f59268-25d4-49f2-bb3a-319ba05cbfc3")
		)
		(fp_line
			(start 1.66 -0.25)
			(end -1.64 -0.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8c76e0b3-5acf-48c1-ac78-af9b3bd53fee")
		)
		(fp_line
			(start 1.66 0.51)
			(end 1.28 0.51)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8a1cfa6d-62f1-4fd6-bc27-f1bab52b94b4")
		)
		(fp_line
			(start 1.66 3.68)
			(end -1.64 3.68)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "06e3b0a1-35f2-44da-807a-8cc3b60a5381")
		)
		(fp_line
			(start 1.66 3.68)
			(end 1.66 0.51)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9f60941b-daef-4091-a1e5-16ad10843b07")
		)
		(fp_line
			(start 2.04 -5.97)
			(end -2.02 -5.97)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d2bc3103-e76f-4ab9-8013-629241878089")
		)
		(fp_line
			(start 2.04 -3.43)
			(end -2.02 -3.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9645fc2e-abb6-4dd8-ab90-beb2244280a7")
		)
		(fp_line
			(start 2.04 -3.43)
			(end 2.04 -5.97)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b35ff119-6a69-4160-9cc3-8fd7b3b874ee")
		)
		(fp_line
			(start 2.04 -0.25)
			(end 1.66 -0.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d00323b6-11c2-402e-8561-05cf71eb2529")
		)
		(fp_line
			(start 2.04 4.32)
			(end -2.02 4.32)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bad68caf-810e-4ee2-979a-4855d842c16b")
		)
		(fp_line
			(start 2.04 4.32)
			(end 2.04 -0.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "110d9a7f-d713-4527-9b1c-c7f63ab9d54e")
		)
		(fp_line
			(start 2.04 6.22)
			(end 2.04 4.32)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "30061278-209c-4e7a-ac47-808915ed6c54")
		)
		(fp_line
			(start 2.04 6.22)
			(end 2.98 6.22)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5f9faf70-3b75-48c8-bb35-ad704783efe8")
		)
		(fp_line
			(start 2.98 -5.97)
			(end 7.05 -5.97)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8161c720-d453-476d-b90d-7148ab9cf2e3")
		)
		(fp_line
			(start 2.98 -3.43)
			(end 2.98 -5.97)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b407fcd2-a71a-42b1-94e2-0f1e81c16d71")
		)
		(fp_line
			(start 2.98 -0.25)
			(end 3.36 -0.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a077e7f6-7b1d-4bed-b781-f6ae0e338d23")
		)
		(fp_line
			(start 2.98 4.32)
			(end 2.98 -0.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5ed3306c-cf60-4fb1-b96b-f25d31dd4c20")
		)
		(fp_line
			(start 2.98 4.32)
			(end 7.05 4.32)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "49974b83-9a1a-4132-ab7b-b637521468d3")
		)
		(fp_line
			(start 2.98 6.22)
			(end 2.98 4.32)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "417bee95-a369-4d2f-9776-bf922e721ab7")
		)
		(fp_line
			(start 2.98 6.22)
			(end 7.05 6.22)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4223d536-5773-487a-93bb-9d947e2f12b1")
		)
		(fp_line
			(start 3.36 -0.25)
			(end 6.67 -0.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "58bcafc8-e959-4fc7-9466-0e60044e053b")
		)
		(fp_line
			(start 3.36 0.51)
			(end 3.74 0.51)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "158397c5-ccf0-4d4c-af07-2e58926244fb")
		)
		(fp_line
			(start 3.36 3.68)
			(end 3.36 0.51)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e5966f07-52bb-452f-8d0f-456d776118bd")
		)
		(fp_line
			(start 3.39 -4.45)
			(end 6.44 -5.08)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4cab474b-9065-45e3-ae3e-eb780cb1223f")
		)
		(fp_line
			(start 3.52 -4.32)
			(end 6.56 -4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9eb7745d-8770-4b69-8eae-4c6cd37c7c69")
		)
		(fp_line
			(start 3.74 -0.25)
			(end 6.28 -0.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7cca55c2-26c7-449d-999e-d3dcb39c07d9")
		)
		(fp_line
			(start 3.74 2.54)
			(end 3.74 -0.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bddaf88f-3d17-45f3-99dd-833bd3ea7671")
		)
		(fp_line
			(start 3.74 2.54)
			(end 6.28 2.54)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "27d3b7aa-4e6b-4bca-9d12-e1dae96278cb")
		)
		(fp_line
			(start 6.28 2.54)
			(end 6.28 -0.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "afbc0678-8b96-4b57-a773-bdda6d38d3f5")
		)
		(fp_line
			(start 6.67 -0.64)
			(end 3.36 -0.64)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "61968f20-de20-45fc-894b-5a43b32bab33")
		)
		(fp_line
			(start 6.67 0.51)
			(end 6.28 0.51)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eb7f28d0-0f04-4bf4-9640-9f583fdd1168")
		)
		(fp_line
			(start 6.67 3.68)
			(end 3.36 3.68)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3217f123-c5ba-4b7f-90a7-fe8546944885")
		)
		(fp_line
			(start 6.67 3.68)
			(end 6.67 0.51)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1e8fa97b-a059-4bcb-9def-9ff882b82646")
		)
		(fp_line
			(start 7.05 -5.97)
			(end 7.05 -3.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "570b0c72-c558-493d-bd5e-fa076b6ff508")
		)
		(fp_line
			(start 7.05 -3.43)
			(end 2.98 -3.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "efe34a21-993a-4754-9fb4-eb01a44f16c1")
		)
		(fp_line
			(start 7.05 -0.25)
			(end 6.67 -0.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eba7812d-0399-4763-a3f4-fd24cb7ef2d4")
		)
		(fp_line
			(start 7.05 -0.25)
			(end 7.05 4.32)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2bde614c-e5fc-41b3-961a-7ed34c3db149")
		)
		(fp_line
			(start 7.05 4.32)
			(end 7.05 6.22)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aa691d5c-98b7-4b67-8c70-96c1356c3402")
		)
		(fp_line
			(start 7.05 6.22)
			(end 7.61 6.22)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3b191a5c-d35b-4db8-b9ff-2aa83b8e8853")
		)
		(fp_line
			(start 7.61 -6.22)
			(end -2.58 -6.22)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a1eb2fb5-60ec-487a-b10e-822965e09188")
		)
		(fp_line
			(start 7.61 -6.22)
			(end 7.61 -3.17)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "86ca4595-9370-46f1-b483-2c709381271e")
		)
		(fp_line
			(start 7.61 -6.22)
			(end 8.11 -6.22)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3e40f710-2666-4d8a-86b1-d5ad4ca47a2c")
		)
		(fp_line
			(start 7.61 -3.17)
			(end 7.61 -1.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "765eb64f-0ce2-481b-bd62-a375364efe28")
		)
		(fp_line
			(start 7.61 -1.65)
			(end 7.61 -0.64)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cb4c48a8-d4e2-4cfb-bdfa-c14dc36fa072")
		)
		(fp_line
			(start 7.61 -0.64)
			(end 6.67 -0.64)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "31873d82-7ac6-415f-b5f3-165b1b2c62f3")
		)
		(fp_line
			(start 7.61 -0.64)
			(end 7.61 4.06)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6743403f-55cc-41f6-9da5-286f1d91e3a1")
		)
		(fp_line
			(start 7.61 4.06)
			(end 7.61 5.21)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9343b39c-3a9c-4fb3-8143-c7bc67413ba1")
		)
		(fp_line
			(start 7.61 5.21)
			(end 7.61 6.22)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f442ca2d-45da-492d-a543-85692b03a927")
		)
		(fp_line
			(start 8.11 -6.22)
			(end 8.11 -1.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "38046375-c8bc-4e15-8d85-4a4867236e28")
		)
		(fp_line
			(start 8.11 -1.4)
			(end 7.61 -1.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fe4d4846-9929-4fb8-8571-4c11076e0f4c")
		)
		(fp_line
			(start 8.11 3.81)
			(end 7.61 4.06)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c85c1d98-240b-4c98-9d65-2fe96abb0c0a")
		)
		(fp_line
			(start 8.11 3.81)
			(end 8.11 5.46)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "40eee14c-4fa4-4528-a5c0-53865fbbfad5")
		)
		(fp_line
			(start 8.11 5.46)
			(end 7.61 5.21)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fb3f351c-18e4-4ab0-b312-1db742e8faec")
		)
		(fp_arc
			(start -1.62 -5)
			(mid -0.05669 -5.772528)
			(end 1.539976 -5.071534)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "94fddb8c-7fd4-4877-a1b6-d24363495d87")
		)
		(fp_arc
			(start -1.42 -4.13)
			(mid -1.718466 -4.559406)
			(end -1.562972 -5.058699)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2cd55029-fbbb-46fb-8d5c-5be029410c04")
		)
		(fp_arc
			(start 1.53 -5.05)
			(mid 1.708693 -4.558754)
			(end 1.485619 -4.086005)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c1df5f19-5617-4a05-a9cc-82cf3467ebb7")
		)
		(fp_arc
			(start 1.53 -4.12)
			(mid 0.02849 -3.628196)
			(end -1.459829 -4.158582)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1d363848-2d26-48cd-93e6-a81ed184f0e3")
		)
		(fp_arc
			(start 3.39 -5)
			(mid 4.949737 -5.764867)
			(end 6.538239 -5.061686)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9f907486-45ae-4d06-b2a3-9a98032aa9d1")
		)
		(fp_arc
			(start 3.58 -4.13)
			(mid 3.281534 -4.559406)
			(end 3.437028 -5.058699)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "16da06d5-51b2-4155-b835-3ab1ee71264c")
		)
		(fp_arc
			(start 6.53 -4.12)
			(mid 5.030583 -3.634318)
			(end 3.547667 -4.168263)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "57e0d509-2345-4aa9-8edf-64a73d8d6e42")
		)
		(fp_arc
			(start 6.54 -5.05)
			(mid 6.715733 -4.551652)
			(end 6.485532 -4.076005)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2b294b81-fe31-4f52-9434-e46de417eb03")
		)
		(fp_text user "${REFERENCE}"
			(at 2.5 -2 0)
			(layer "F.Fab")
			(uuid "5bb1c603-eb4b-423d-ae7c-2fae7160f1b3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.98 3.96)
			(drill 1.32)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(BT1-+)")
			(pinfunction "+")
			(pintype "passive")
			(uuid "276cb00a-7287-4eef-bd02-2df61e8e69a1")
		)
		(pad "2" thru_hole oval
			(at 5 0)
			(size 1.98 3.96)
			(drill 1.32)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "-")
			(pintype "passive")
			(uuid "93644025-ee30-43f4-a0af-c16131d1cf28")
		)
		(model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_Altech_AK300-2_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-3"
		(layer "F.Cu")
		(uuid "e716de49-eda1-409f-a187-cbcb24871b5e")
		(at 109.55 89.3625 90)
		(descr "SOT, 3 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178D.PDF inferred 3-pin variant), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q1"
			(at 0 -2.4 90)
			(layer "F.SilkS")
			(uuid "1d923d6e-2302-4878-b8a7-07319c0c5807")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "IRLML6244"
			(at 0 2.4 90)
			(layer "F.Fab")
			(uuid "9fe9baad-f722-4775-ac93-ebe60d745b2d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-3"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b4813dd5-4a19-4e0e-b985-bcd3caf5dcc4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "29b5fac4-20b0-4324-837f-0e6d6137583d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "30A Id, 50V Vds, N-Channel Power MOSFET, TO-220"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0097a8e1-3432-4300-9381-8408acb1e5d5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/15c2dde6-2c28-40a3-b434-60eca1b941fe")
		(sheetfile "led-controller.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -1.56)
			(end 0.8 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4dd4d8f9-7a77-418d-b5c7-704a19987ed1")
		)
		(fp_line
			(start 0 -1.56)
			(end -0.8 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c19dfd92-a0bf-4dd3-ad01-98d95bf5575b")
		)
		(fp_line
			(start 0 1.56)
			(end 0.8 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "655f6ae8-6bdf-4c24-a56f-0d6b26ffd51b")
		)
		(fp_line
			(start 0 1.56)
			(end -0.8 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7310afe4-0a67-461a-b946-2d7226993b91")
		)
		(fp_poly
			(pts
				(xy -1.3 -1.51) (xy -1.54 -1.84) (xy -1.06 -1.84) (xy -1.3 -1.51)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "59e4545d-4ccc-4ecc-b6fb-2e45f7bb6e6e")
		)
		(fp_line
			(start 2.05 -1.7)
			(end -2.05 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3ba65246-3d05-44c3-9bcb-e8907dc1f6b8")
		)
		(fp_line
			(start -2.05 -1.7)
			(end -2.05 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f8a49f01-7df1-464a-998b-3b1225d263b1")
		)
		(fp_line
			(start 2.05 1.7)
			(end 2.05 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f5dbb2fc-a45c-41e7-8ce4-c824eed42ef6")
		)
		(fp_line
			(start -2.05 1.7)
			(end 2.05 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e48bb561-c78c-483c-98bb-4134abc2b794")
		)
		(fp_line
			(start 0.8 -1.45)
			(end 0.8 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "839538c5-d033-4504-b431-b836ecf37d4a")
		)
		(fp_line
			(start -0.4 -1.45)
			(end 0.8 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "62583711-df7e-4d3b-8085-4e7c4f630e55")
		)
		(fp_line
			(start -0.8 -1.05)
			(end -0.4 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a35e5e24-7976-4a71-86ea-fb7d81ca8429")
		)
		(fp_line
			(start 0.8 1.45)
			(end -0.8 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a1caa5d0-990a-45af-8052-02eb20ad601c")
		)
		(fp_line
			(start -0.8 1.45)
			(end -0.8 -1.05)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "68d89f43-3417-47ad-a978-29a975a85492")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "bec2ee46-7d13-424b-8283-a7113718bcd2")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "Net-(J2-Pin_3)")
			(pinfunction "G")
			(pintype "input")
			(uuid "e04a0bc0-546e-4aee-be1e-cd0be93ed989")
		)
		(pad "2" smd roundrect
			(at -1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Net-(J1-Pin_2)")
			(pinfunction "D")
			(pintype "passive")
			(uuid "79892c33-45aa-4e93-a8aa-37b874e2e9a0")
		)
		(pad "3" smd roundrect
			(at 1.1375 0 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "S")
			(pintype "passive")
			(uuid "28f4a5b1-a901-49e6-be17-77b7d96afb58")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-3.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-3"
		(layer "F.Cu")
		(uuid "f727b156-2bca-4dc2-a39f-3cef4443f739")
		(at 99.95 89.3625 90)
		(descr "SOT, 3 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178D.PDF inferred 3-pin variant), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q3"
			(at 0 -2.4 90)
			(layer "F.SilkS")
			(uuid "a396ae8c-7db6-47f4-8ac4-fc0e51374518")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "IRLML6244"
			(at 0 2.4 90)
			(layer "F.Fab")
			(uuid "09ddc3e9-64d6-4c1c-a809-aa3d8bb1d05e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-3"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "32d04bc1-151d-42a4-9914-cc164fe3c188")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4d22843b-ade2-4d84-a14d-a07314e588e8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "30A Id, 50V Vds, N-Channel Power MOSFET, TO-220"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f107048c-00eb-4fb4-b117-8cbc30cb750d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/9eef009a-860c-4127-8cf2-cea04ca1ace4")
		(sheetfile "led-controller.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -1.56)
			(end 0.8 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c82d68f2-4015-4ada-8998-e710d1aad5da")
		)
		(fp_line
			(start 0 -1.56)
			(end -0.8 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dfe591c1-4565-43d2-a31b-c1b848eaa139")
		)
		(fp_line
			(start 0 1.56)
			(end 0.8 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5d6e9405-6d3b-4632-9947-e8335ab6a67b")
		)
		(fp_line
			(start 0 1.56)
			(end -0.8 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "17931bbf-fa17-4296-89dc-7f38f82c3f5e")
		)
		(fp_poly
			(pts
				(xy -1.3 -1.51) (xy -1.54 -1.84) (xy -1.06 -1.84) (xy -1.3 -1.51)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "02b1ecd6-5103-4d6a-8222-e3260368a154")
		)
		(fp_line
			(start 2.05 -1.7)
			(end -2.05 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fc1860f3-9668-40a7-aa6e-50d2f06a1a97")
		)
		(fp_line
			(start -2.05 -1.7)
			(end -2.05 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d8a4f5d3-1abd-4217-a23f-89b1c4d2ee27")
		)
		(fp_line
			(start 2.05 1.7)
			(end 2.05 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3e2ef7fd-7b8e-4735-a430-8061cead3d9e")
		)
		(fp_line
			(start -2.05 1.7)
			(end 2.05 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "020d5765-e032-4b41-9fb3-c6dad95d0672")
		)
		(fp_line
			(start 0.8 -1.45)
			(end 0.8 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "32188e6e-d181-42b2-bf27-f488e3e5cc53")
		)
		(fp_line
			(start -0.4 -1.45)
			(end 0.8 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f1f8d62f-b8c7-4116-a147-64222c5de517")
		)
		(fp_line
			(start -0.8 -1.05)
			(end -0.4 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a3a468a1-e096-425f-a764-88d466c1fe4b")
		)
		(fp_line
			(start 0.8 1.45)
			(end -0.8 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "46943bc3-9461-4eea-bd8c-605550c50f3b")
		)
		(fp_line
			(start -0.8 1.45)
			(end -0.8 -1.05)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "40459e7c-42fe-49fe-b0d4-2be530d363bd")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "ae95d20d-2e92-4c68-b6a9-a6fe6c261b9a")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "Net-(Q3-G)")
			(pinfunction "G")
			(pintype "input")
			(uuid "8d00d9a2-a976-4bf3-820a-49e162084104")
		)
		(pad "2" smd roundrect
			(at -1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "Net-(J1-Pin_4)")
			(pinfunction "D")
			(pintype "passive")
			(uuid "619031f6-6d01-4290-bb74-0d515ff74d5d")
		)
		(pad "3" smd roundrect
			(at 1.1375 0 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "S")
			(pintype "passive")
			(uuid "9a7cc638-14ff-42d0-9535-1a6ce8bf1daf")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-3.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 96.056 75.78)
		(end 124.968 109.412)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "Edge.Cuts")
		(uuid "2543f2c9-748e-43f4-83ac-fa090cdbebfa")
	)
	(segment
		(start 109.22 107.95)
		(end 109.23 107.96)
		(width 0.3)
		(layer "F.Cu")
		(net 8)
		(uuid "6d0d4555-9f25-43aa-8440-7ae225661d64")
	)
)
